Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Filter Width

Stores the default value of the filter width used in conjunction with the Median and Weighted average laser sensor filters. See the "Laser Probe Toolbox: Laser Filtering Properties tab" topic in the PC-DMIS Laser documentation for more information. documentation).

Entry Name: SensorFilterWidth

Entry Type: Real Number to specify filter width in pixels. Default value is 0.