Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Vision Par Calibration Use Bridging

This entry determines whether or not the series of concentric circles are measured and bridged (or linked) together during the parfocal high calibration in order to automatically correct for a measured concentricity error in the calibration standard. If this entry is set to FALSE then it assumes the standard is perfect.

Important: If a fovcert.dat file is used to provide concentric circle XY position certification data then this bridging is not done, even if this value is set to TRUE.

Entry Name: ProbeQualVisionParCalibrationUseBridging

Entry Type: Boolean value indicating whether or not bridging (or linking) is used during parfocal high calibration. The default value is TRUE.