Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Void Detection

This option determines whether Void Detection is used in the measurement of the following Auto features:

- Auto Surface Point

- Auto Edge Point

- Auto Line

- Auto Plane

- Auto Circle

- Auto Round Slot

- Auto Cylinder

- Auto Cone

Void Detection prevents hits from being taken in empty spaces (such as holes).

Entry Name: DccVoidDetection

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 1.

Note: PC-DMIS can use void detection only if your hardware key (or portlock) has been programmed with the IP measure item.