Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Trigger Force

Allows you to enter the force at which a measurement reading is taken. For a normal deflection mode (DFL) probing cycle, this is the force at which the Actual Point (APT) will be calculated and returned to PC-DMIS. Not all analog probes/controllers use this input.

Entry Name: ProbeTriggerForce

Entry Type: Real Number specified in newtons. Default value is 0.06.