Current Help System: PC-DMIS Settings Editor (View Core Help)

### DCC Targ IJK_2

Provides the default "K" value for various IJK vectors that are used in the creation of Auto Features using an NC-100 video probe. The value is applied to different vector types (Surface, Edge, etc.) depending on the auto feature type.

Note: Because of the variance between auto features and how this value is applied, it is best to alter this value from the Auto Feature dialog box within PC-DMIS.

Entry Name: DccTargIJK_2

Entry Type: Real Number to specify the K vector value. Default value is 0.