Current Help System: PC-DMIS Settings Editor (View Core Help)

### Edge Point CG Gray Sum Max

Provides the maximum pixel intensity beyond which pixels exceeding this value will not be used. This value is used when measuring laser edge point features using the Gray Sum locater type.

Entry Name: EdgePoint_CGGraySumMax

Entry Type: Whole Number specifying maximum pixel intensity. Default value is 300.