Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Manual Fine

Specifies whether this option is TRUE (1) or FALSE (0). When set to TRUE (1) PC-DMIS will switch to DCC mode after a manual point is measured. This allows for normal deflection probing cycle to be used when the probe is moving away. This may result in slower manual probing but improves accuracy.

Not all analog probes/controllers support this mode of manual probing. In those cases, PC-DMIS ignores this check mark. Your CMM controller's manufacturer will know if your controller supports this option.

Entry Name: ProbeManualFine

Entry Type: Whole Number to specify TRUE (1) or FALSE (0). Default value is 0.