Current Help System: PC-DMIS Settings Editor (View Core Help)

### Probe Qual Analog Disk Use Plane On Bottom

PC-DMIS will do one of the following Disk Stylus calibration based on this setting:

- When this entry is set to 1, PC-DMIS takes four hits on top of the sphere using a circular pattern on the bottom of the disk stylus and calculates a plane from it. Measuring a plane helps ensure that the hits for calibrating the face are oriented properly to reflect the actual plane of the disk. This is the default for the traditional calibration method using discrete hits.

- When this entry is set to 0, PC-DMIS does not attempt to measure a plane on the bottom of the disk's face. Instead it uses the design orientation of the disk. This is the default for the Renishaw scan-based calibration.

Entry Name: ProbeQualAnalogDiskUsePlaneOnBottom

Entry Type: Whole Number specifying TRUE (1) or FALSE (0). Default value is TRUE (1).