Current Help System: PC-DMIS Vision (View Core Help)

#### Circle Field Definitions with NC-100

Many of the definitions are already covered in the "Circle Field Definitions" topic in the "Creating Auto Features" section. The following definitions are added or changed when using a NC-100 video probe :

SHOWHITS = This is a toggle field. It toggles from YES to NO and determines if hits will be displayed with this feature.

SHOWALLPARAMS = This is a toggle field. It toggles from YES to NO as to displaying all the parameters on the feature.

THEO_THICKNESS = This editable value indicates the keyed in thickness of the part. Positive or negative values can be used.

ACTL_THICKNESS = This value indicates the keyed in offset thickness of the measured data. Positive or negative values can be used.

THEO / = This value represents the theoretic feature location. DNOM is the diameter 's nominal value.

ACTL /= This value represents the measured hit . DNOM is the diameter's measured value.

TOG2 = This toggle field switches between IN and OUT. PC-DMIS will determine the type of circle that is measured based on the location of the probe when taking the hit. (Inside a circle = IN, outside a stud = OUT.) Only available with Hole feature type.

TOG3 = This toggle field switches between LEAST_SQR, MAX_INSC, MIN_CIRCSC, MIN_SEP, and FIXED RAD. Only available with Hole feature type.

NUM HITS = This editable value must be an integer that is greater than two. Only available with Hole feature type.

See the "Common Auto Feature Dialog Box Options" topic in the "Creating Auto Features" section for general guidelines on measuring all Auto Feature types.