TOG19 = EDGE TYPE
This toggle field switches between the available types of edge detections. They are: DOMINANT EDGE, SPECIFIED EDGE, NEAREST NOMINAL, or MATCHING EDGE. See "Probe Toolbox: Hit Targets tab" for more information. This value is not used for a SURFACE POINT. n1 = Edge strength threshold to be used during the teach process. All edges that are assigned a ‘strength’ that is below this threshold will be ignored when looking for an edge. Values should fall between the range of 0 and 255. n2 = Hit target direction (--> or <--). n3 = Specified Edge - This parameter defines the Nth edge to be used for the specified edge detection method. Currently allows a number between 1-10 to be entered. n4 = This value determines if the edge that is being viewed and found goes from black to white "[|] ->[ ]", white to black "[ ] ->[|]", or either "[?] ->[?].