Current Help System: PC-DMIS Vision (View Core Help)

#### Feature Type list

The Feat Type list provides you with the following feature types:

For Edge Points

NORMAL = This is the Normal edge type measurement that occurs at the surface height of the edge.

DELTAZ = This option allows the measurement of an edge at a specified depth in respect to the plane on which the surface lies.

HIGH POINT = This option allows the measure of an edge at the maximum value in a specified direction.

BIGHOLE = This option allows the measure of an edge used to measure a part of a hole bigger than the sensor field of view.

For Characteristic Points

From the Feat Type list you can select the available types of characteristic points. These include:

CHAR 1 = This type of feature allows the measurement of two points (one on each surface) at a given indent from the intersection of two planes.

CHAR 2 = This type of feature measures the point at the intersection of two planes.