Current Help System: PC-DMIS Vision (View Core Help)

## Using Vision Gages

The gage functionality of PC-DMIS Vision provides a simple method to compare actual part geometry to a gage. For example, overlay a gage (whose diameter is set to exactly 1.0mm) to an actual part hole to compare its size.

Considerable functionality is available with gages. This section is provided to give an example of the usage of each type of gage. For detailed information in the available buttons and options, see "Probe Toolbox: Gage tab".

The six available gages are:

Cross Hair Gage

Circle Gage

Rectangle Gage

Protractor Gage

Radius Chart Gage

Grid Chart Gage

The selected gage can be centered within the FOV at any time by pressing Center Gage from the Gage tab of the Probe Toolbox.

For each gage example the HexagonDemoPart.igs demo part is used. See "Importing the Vision Demo Part".