Current Help System: PC-DMIS Vision (View Core Help)

#### Specific Functions for Flush and Gap Features

There are a few values that are specific to the Flush and Gap Auto Feature dialog box. They are:

- Depth - Defines the distance below the surface of the fixed side that PC-DMIS will measure the gap & flush. This becomes available if you select GAP DELTAZ from the Feat Type list.

- Depth2 - Defines the distance below the surface of the moving side that PC-DMIS will measure the gap & flush. This becomes available if you select GAP DELTAZ from the Feat Type list.

- Gap - Displays the gap of the Gap & Flush.

- Flush -Displays the Flush of the Gap & Flush.

- Type - The RIGHT option and the LEFT option define the fixed side of the Gap & Flush measurement. In Gap & Flush measurements you need to define one side as the fixed (or nominal) side. The fixed side becomes the datum against which the other side is measured.