Current Help System: PC-DMIS Vision (View Core Help)

### How AutoTune Execution Works

When you execute your part program in AutoTune execution mode, PC-DMIS Vision steps you through the program, feature by feature.

It performs a test measurement on each feature and then displays the AutoTune dialog box for that feature, indicating what has been changed.

You then have the option to apply one or more of those changes to one or more subsequent features in the part program.

Once you are satisfied with the feature and you click Continue, PC-DMIS Vision then tests the next feature. It continues doing this until the entire part program has been executed in AutoTune execution. You can also use the Apply and Finish button at any time to apply changes to the selected features and end the AutoTune execution sequence.

Once you finish executing the part program in AutoTune execution, you can return to PC-DMIS's regular execution mode.