Current Help System: PC-DMIS Vision (View Core Help)

### Machine Options: Pendant tab

Machine Options dialog box – Pendant tab

The Pendant tab, available on selected machines, allows you to define the speed parameters for your manual control box. Your manual control box is the hardware component PC-DMIS Vision uses to manually drive your Vision probe toward and away from features you want to measure. This manual control is either a joystick or a joystick and a trackball.

Most optical systems provide just a joystick while some systems provide both a joystick and a trackball. You can change the speed that the optical probe will use by altering the values in the boxes provided. The speed is listed in mm per second.

More:

Joystick

Trackball