#### To Use Looping:

1. Select Insert | Flow Control Command | Looping from the menu bar. The Looping Parameters dialog box will appear.

2. Make any necessary changes to the boxes.

3. Select parameters as needed (i.e. Number of Parts, Start Number, Skip Number, offsets in XY or Z, Angle).

4. Place the cursor in a location in the Edit window where you want to begin the loop.

5. Select the OK button.

The Edit window command line for looping reads:

VARNAME = LOOP/START, ID = Y/N, NUMBER = 0, START = 1, SKIP = ,
OFFSET: XAXIS = 0, YAXIS = 0, ZAXIS = 0, ANGLE = 0

Note: To complete the looping procedure, you must have an End Loop command inside the Edit window. PC-DMIS will loop Edit window commands that the LOOP/START and LOOP/END commands encompass. See "End Loop" for more information.