### Basic Measurement Format for a Point

The only number of hits for a point is one. | Feature_name=FEAT/POINT,TOG1 THEO/TX,TY,TZ,TI,TJ,TK ACTL/X,Y,Z,I,J,K MEAS/POINT,TOG3 HIT/…
ENDMEAS/

TOG1= This field can be toggled between RECT / POLR.

TOG3= This list the number of hits that PC-DMIS should take to measure this feature. Since a point can only have one point, you cannot edit this value for this feature.

...= A single hit is entered at the ellipsis.