#### Rotate to a Line between Two Circles

To rotate to the line between two circles, select two circles in the Feature List box and click the Rotate button. As in the other type of rotate, select the axis to rotate, the axis to rotate around, and enter the offset value (if desired).

The Edit window command line for this option reads:
ALIGNMENT/ROTATE_CIRCLE,ID, ID

Changeable fields: "ID"

This is one of the two ids to which to rotate.