## Migrating Part Programs Between Machines Using PH10 and Tesa Star M Probes

In version 4.3 and higher, in the Option section of the PC-DMIS Settings Editor, PC-DMIS provides the AutoAdjustTesaM5Degrees registry entry to assist in migrating part programs between two machines that use a PH10 probe on one machine and a Tesa Star M probe on the other. Both machines must have probe files with the same name (although the probe files themselves will be different).

- If the registry entry is set to 1, when a part program that was created initially on one of these machines is then loaded onto the other, PC-DMIS will convert any active TIP/ commands to the closest AB tip angle based on the index increment. If any angles are converted, a message box appears displaying them.

- If the registry entry is set to 0, PC-DMIS will not perform this angle adjustment.

The default value is 1.