#### Use DMIS Polar Convention

With this option selected, polar angles will follow standard DMIS Polar Convention.

- XY Plane (PLUS Z or MINUS Z) coordinate 'a' is the angle from the x-axis towards the y-axis.

- YZ Plane (PLUS X or MINUS X) coordinate 'a' is the angle from the y-axis towards the z-axis.

- ZX Plane (PLUS Y or MINUS Y) coordinate 'a' is the angle from the z-axis towards the x-axis.