### Keying in Probe Depth

It is sometimes necessary to set the probe at some specific location in space. To do this:

1. Click on the X, Y, Z portion of the status bar while in Program mode (or select the Operation | Move To option described in the "Inserting Move Commands"section ).

2. The Auto Move Point dialog box will appear. The default setting indicates the probe's current location.

3. Change the X, Y, Z to the desired values. By selecting the Store Move check box, the MOVE POINT command can be added to the program. You also have the ability to select the Increment moves check box and the OK to Move check box.

4. Once the new X, Y, or Z values are entered, click on Done and PC-DMIS will move the animated probe to the new position.