#### References of Type Double

The following reference expressions are available:

Valid Extensions for Feature References of Type Double by Example

Format: <Feature Id>.<Extension> -> CIRCLE1.X

CIRCLE1.X Measured X Value of CIRCLE1
CIRCLE1.Y Measured Y Value of CIRCLE1
CIRCLE1.Z Measured Z Value of CIRCLE1

CIRCLE1.TX Theoretical (Nominal) X Value of CIRCLE1
CIRCLE1.TY Theoretical (Nominal) Y Value of CIRCLE1
CIRCLE1.TZ Theoretical (Nominal) Z Value of CIRCLE1

LINE1.SX Measured X Value of the Startpoint of LINE1
LINE1.SY
LINE1.SZ

LINE1.TSX Theoretical X Value of the Startpoint of LINE1
LINE1.TSY
LINE1.TSZ

LINE1.EX Measured X Value of the Endpoint of LINE1
LINE1.EY
LINE1.EZ

LINE1.TEX Theoretical X Value of the Endpoint of LINE1
LINE1.TEY
LINE1.TEZ

POINT.I Measured I Component of Vector for POINT
POINT.J
POINT.K

POINT.TI Theoretical I Component of Vector for POINT
POINT.TJ
POINT.TK

FEAT1.TYP The type of the feature (i.e. circle, slot, cone). This can be used to change the type of a generic feature (Assign/ Gen1.TYP = Feat1.TYP).

FEAT1.ALL Refers to all elements of the feature. This is valuable for copying information to a generic feature. (Assign/ Gen1.ALL = Feat1.ALL)

Surface Vector

EDGE.SURFI

EDGE.SURFJ

EDGE.SURFK

EDGE.TSURFI

EDGE.TSURFJ

EDGE.TSURFK

Angle Vector

CIR.ANGI

CIR.ANGJ

CIR.ANGK

CIR.TANGI

CIR.TANGJ

CIR.TANGK

Radius

CIRCLE1.R

CIRCLE1.TR

CIRCLE1.RAD

CIRCLE1.TRAD

CIRCLE1.RADIUS

CIRCLE1.PR – Polar Radius

CIRCLE1.TPR – Theoretical Polar Radius

CIRCLE1.TRADIUS (Only the First Characters are significant)

Diameter

CIRCLE1.D

CIRCLE1.TD

CIRCLE1.DIAM

CIRCLE1.TDIAM

CIRCLE1.DIAMETER

CIRCLE1.TDIAMETER (Only the first characters are significant)

Angle

CONE.A

CONE.TA

CONE.ANG

CONE.TANG

CONE.ANGLE

CONE.TANGLE

CONE.PA – Polar Angle

CONE.TPA – Theoretical Polar Angle (Only the First Characters are significant)

Length

LINE.L

LINE.TL

LINE.LEN

LINE.TLEN

LINE.LENGTH

LINE.TLENGTH (Only the First Characters are significant)

Height

CYLINDER.PH – Polar Height

CYLINDER.TPH – Theoretical Polar Height

Radius, Angle, Height

POINT.RAH – Point with Measured Radius, Angle, and Height

POINT.TRAH – Point with Theoretical Radius, Angle, and Height

Valid Extensions for Dimension Reference of Type Double by Example

Format: <Dimension ID>.<AXIS>.<Dimension Element> -> DIM1.X.NOM

DIM1.X.NOM | The Nominal Value for X Axis Location of DIM1
DIM1.X.MEAS | The Measured Value for the X Axis Location of DIM1
DIM1.X.MAX | The Max Deviation for X Axis Location of DIM1
DIM1.X.MIN | The Min Deviation for X Axis Location of DIM1
DIM1.X.PTOL | The Plus Tolerance Value for the X Axis Location of DIM1
DIM1.X.MTOL | The Minus Tolerance Value for the X Axis Location of DIM1
DIM1.X.DEV | The Deviation on the X Axis Location of DIM1
DIM1.X.OUTTOL | The Out of Tolerance value on the X Axis Location of DIM1
DIM1.Y.NOM | The Nominal Value for the Y Axis Location of DIM1
DIM1.Z.DEV | The Deviation on the Z Axis Location of DIM1
DIM3.PA.MEAS | The Measured Value for the Polar Angle Location of DIM3
DIM4.M.PTOL | The Plus Tolerance Value for the M Axis of DIM4
*DIM4.PTOL | The Plus Tolerance Value for the M Axis of DIM4 (See Note under "Valid Axes " below).
DIM5.BTOL | The Bonus Tolerance Value where DIM5 is a Position.

Valid Axes:

X, Y, Z, D, R, A, T, V, L, PR, PA, M, PD, RS, RT, S, H, DD, DF, TP

Note: * Dimensions that have only one axis by definition (i.e. roundness, concentricity, etc.) can omit the axis qualifier. If the axis qualifier is used, note that all of these types of dimensions (that have only one axis) use the M Axis qualifier with the exception of 2D and 3D angle dimensions, which use the A Axis qualifier.

Valid Extensions for Alignment References of Type Double by Example:

Format: <Alignment ID>.<Alignment Axis or Origin>.<Alignment Axis or Origin Component> -> A1.ORIGIN.X

A1.ORIGIN.X | X Component of alignment A1’s measured origin
A2.ORIGIN.Y | Y Component of alignment A2’s measured origin
A1.ORIGIN.Z | Z Component of alignment A1’s measured origin
A1.XAXIS.I | I Component of alignment A1’s measured X axis
A1.YAXIS.J | J Component of alignment A1’s measured Y axis
A1.ZAXIS.K | K Component of alignment A1’s measured Z axis
A1.CORIGIN.X | X Component of alignment A1’s origin based on theoretical (C is for CAD) data
A1.CXAXIS.J | J Component of alignment A1’s X axis based on theoretical (C is for CAD) data