#### Meas All Always

If you select the Meas All Always check box, PC-DMIS will re-execute a portion of the current part program at least once in DCC mode. The portion that is re-executed depends on the Start Label (see "Start Label")

If you provide a start label,

- PC-DMIS will re-execute from that defined label to the ALIGNMENT/START command that contains the currently executing iterative alignment command.

If you don't provide a start label,

- PC-DMIS will begin this re-execution from the first feature measured in the program that is used by the iterative alignment command.

- If the first feature has stored move points preceding it, then PC-DMIS will also execute these move points.

- The re-execution will continue until the last measured feature used by the iterative alignment command.

- If there are any stored moves after this command, they will not be executed.

Once the re-execution finishes, PC-DMIS will recalculate the alignment and test any measured input points to see if they are all within the tolerance radius specified in the Point Target Radius value.

- If they are all in target, re-execution does not need to continue and PC-DMIS will consider the iterative alignment command complete.

- If any points missed the target area, then the same portion of the program will be re-executed as described above.