### Tolerances for Surface Profile Dimensions

This dimension type is considered either one sided, meaning a single positive value tolerance is applied, or two sided, meaning upper and lower tolerance values are applied.

- If the Form Only option has been selected, only a plus tolerance can be applied.

- If the Form and Location has been selected, the profile dimension can be one sided or two sided.

More:

Plus Tolerance

Minus Tolerance