### TN - Enable Touch Probe

The TN command sets the touch mode to on, re-enabling the touch probe previously disabled with the TF command. If a three-axis analog probe (e.g., the Renishaw SP-600) is in use, then the soft probe is disabled (see the BF command).

Command Format

MLString "TN"

Example

1. MLString "TN"

Input

None.

Results

The touch probe is enabled during all moves.

Skip Action

Executes even when inside a skipped block.

Error Messages

- MLB-090
  DCC is not available.