#### XYZ Move

Move area

The Move area contains XYZ boxes that display the X, Y, and Z nominal for the position of the MOVE/POINT or the increment distance of the MOVE/INCREMENT command.

To change the X, Y, or Z values:

1. Select the field you want to change.

2. Type a new value.

After a new value is entered, PC-DMIS will draw the animated probe at the new location. This indicates the location of the stored move. When the Create button is clicked, PC-DMIS will insert the Move command and position the CMM to the location specified. If you created an offset move, it will update the values in the XYZ boxes to match the computed offset location.

The Cartesian/Polar icon switches the display of the X, Y, and Z values between the Cartesian and Polar coordinate systems. The XYZ labels will change to display RAH when switching to Polar.