Current Help System: Direct CAD Interfaces (View Core Help)

Example of the Pcdmis.dat File on a UNIX Workstation

$ PC-DMIS/CATIA Interface

IP=205.158.132.244;
(Note: IP address of the UNIX workstation)

PORT=5555;
(Note: use same port for both UNIX and Windows)

PORT2=5556;
(Note: this port is just used on the UNIX side for inter-process communication. This is optional)

DEBUG;
(This is optional)

EXIT;
(This is optional)