Current Help System: Direct CAD Interfaces (View Core Help)

### Step 1: Installing PC-DMIS

First, you need to install PC-DMIS. To install PC-DMIS, follow this procedure:

1. Plug your PC-DMIS portlock (also known as a dongle) into the printer port of your PC.

2. Insert the PC-DMIS CD-ROM into your CD-ROM drive.

3. Using Windows Explorer, open the directory containing the CD-ROM and then navigate to the setup.exe application for PC-DMIS.

4. Double click (execute) the file setup.exe.

5. This will activate the PC-DMIS installation sequence.

6. Follow the on-screen instructions until PC-DMIS is installed.

This completes the PC-DMIS installation.