Current Help System: PC-DMIS Fixturing (View Core Help)

#### Volume Definition Tab

Volume Definition - Dual Arm Setup

Measure all data (Read Position) For Arm 1 and Arm 2. Click Take Hit to measure the height of the base plate to which the fixturing components are attached. Read Position for Arm 2 should be done from the Master computer related to Arm1 only. When reading an Arm 2 position, remember to switch to Arm 2 (green icon on Active-Arms/Multiple Arm Toolbar).