Current Help System: PC-DMIS Fixturing (View Core Help)

### Setup Dual Arms with Fixturing Setup Dialog Box

This method should be used when your machine is available to read positions to collect measured data. Information for the Volume Definition and Mount Points tabs are discussed here. See the ”Fixturing Setup: Display Options” section for information about the Display Options tab.

Note: The Display options tab is the same as it would be for a single arm configuration.

More:

Volume Definition Tab

Mount Points Tab