Current Help System: PC-DMIS Laser (View Core Help)

#### Initial Touch Vector (InitVec)

The values that are displayed in the Initial Touch Vector row indicate the vector PC-DMIS will use to take the first touch in the scanning process.

To edit the I, J, K Initial Touch vector:

1. Double click on InitVect in the vector column. The Edit Scan Item dialog box appears.

2. Change the values.

3. Click the OK button. The dialog box will close.