Current Help System: PC-DMIS Laser (View Core Help)

### Creating a Pointcloud/CAD Alignment:

The first step in the alignment process is to perform a rough alignment to bring the pointcloud close enough to CAD (if not already close) to be able to refine the alignment further if needed. There are three types of refinements: UNIFORM, RANDOM and FACE. The Pointcloud/CAD Alignment dialog box can be used for the purpose. It contains the following main areas:

- COP

- Rough Alignment

- Refined Alignment