Current Help System: PC-DMIS Laser (View Core Help)

#### Generate

The Generate button is available only for DCC scans using CAD data.

After the boundary points for a scan has been defined, click the Generate button. PC-DMIS will slice the CAD with the plane defined by the start point and cut vector and then generate the theoretical points from the curve defined by this slice. If the Create button is then clicked, PC-DMIS inserts a scan with nominal hit data will be inserted into the part program.