Current Help System: PC-DMIS NC (View Core Help)

### Part Programs for Stacked Rotary Tables

To create a part program that uses rotary table motion from both of the stacked rotary tables:

1. Select the Edit | Preferences | Rotary Table Setup menu option to open the Rotary Table Setup dialog box.

2. Add a Move Rotary Table command (Insert | Move | Rotary Table) to the part program.

3. Update the Rotary Table W and Rotary Table V axis positions as needed.

4. Create the CNC (.cnc) file in the usual way to include rotary table commands (see "Step 4: Create a NC Program File"). Rotary Table moves are inserted as G01 commands in the CNC file. PCDMIS will correct the coordinates of each move and measurement point.

5. Start the PC-DMIS NC Server Program (see "Step 5: Start the PC-DMIS NC Server Program").

6. Upload the program (see " Step 6: Load the NC Program File" to the controller as usual.

7. Execute the program (see "Step 7: Execute the NC Program File"). Note the points returned in the journal file are appended with the W axis angle followed by the V axis angle.