Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Shutter Time To Fire On Fov Entry

This value provides the delay (in milliseconds) that PC-DMIS waits before firing of the point detection command for an ROI (Region of Interest) that was not entirely in the FOV has just entirely entered the FOV.

This value is only evaluated when "AutoShutterEnable" is set to TRUE (1). If the stage is not stable, then point detection is not reliable.

This value relates to the Movement detected settle in the Live View Setup dialog box. See the "Setting up the Live View" topic in the PC-DMIS Vision help file.

Entry Name: AutoShutterTimeToFireOnFovEntry

Entry Type: Whole Number to specify milliseconds. Default value is 3000.