Current Help System: PC-DMIS Settings Editor (View Core Help)

### Wrist Start B

Provides the starting B angle used for the calibration of your PHS wrist device (where the phs cannot rotate through). As part of the calibration process, you need to calibrate wrist positions in a pattern of at least three A angle positions by at least three B angle positions for a total of nine sphere measurements.

Entry Name: WristStartB

Entry Type: Real Number to specify the starting B angle. Default value is -180.