Current Help System: PC-DMIS Settings Editor (View Core Help)

## USER_NC Sensor Settings

This section of the PC-DMIS Settings Editor allows you to set parameters used with NC Laser machines. Your portlock must be programmed with the proper Laser functionality in order for this section to appear.

More:

AutoAdjustProbeMaxAngle

AuxLens

CGPercentage

CGThreshold

Extrusion

ExtrusionOn

FlatnessTolerance

DeviationLimit

HotSpotErrorEstimate(XYZ)

IntensityThreshold

MaxMeasureDistance

MaxSpan

MaxTrackDistance

MinMeasureDistance

MinTrackDistance

PointCloudID

Projector

QualityThreshold

RegularSpacing

RingBandOn

RingBand_Inner

RingBand_Outer

RowDensity

RowOverlap

RowOverscan

SensorClipLeftPercent

SensorClipLowPercent

SensorClipRightPercent

SensorClipUpPercent

SensorDensity

SensorExposure

SensorFilterWidth

SensorFreq

SensorFrequency

SensorGain

SensorIntensity

SensorMinNeighbor

SensorNeighborNum

SensorOffset

SensorPointsDensityType

SensorSamples

SensorTolAbove

SensorTolBelow

SensorTolRight

UpperBound

Weight(1-9)