Current Help System: PC-DMIS Settings Editor (View Core Help)

### Sensor Clip Low Percent

Provides the bottom edge of the clipping plane as a percentage of your laser sensor's field of view. The clipping plane allows you limit the amount of data that is collected form your laser sensor. For example, a value of 15 would eliminate the first fifteen percent from the bottom edge of the sensor's entire field of view, while a value of 0 will use all data down to the bottom edge of the sensor's field of view.

Entry Name: SensorClipLowPercent

Entry Type: Real Number to specify percentage. Default value is 0.