Current Help System: PC-DMIS Settings Editor (View Core Help)

### PICS Differential Switch Bit

In order to automate probe changes between touch trigger and Perceptron probes on PH10 wrists you must specify the bit used to switch the PICS input to the differential input. This value should only need to be set once and for now the defaults should work for all DEA/B&S machines.

Entry Name: PICSDifferentialSwitchBit

Entry Type: Whole Number to specify the switch bit. Default value is 6.

Administrator permission is