Current Help System: PC-DMIS Settings Editor (View Core Help)

### Min Delta Between Points In MM

Allows you to reduce the measured data by deleting hits that are closer than the distance specified. The reduction of hits happens as data comes from the machine. PC-DMIS only keeps the points that are set apart by more than the specified increments.

Entry Name: MinDeltaBetweenPointsInMM

Entry Type: Real Number to specify distance in MM. Default value is 2. The default value is "0" when using an portable arm machine.