Current Help System: PC-DMIS Settings Editor (View Core Help)

### Include Util Macros

When this value is set to TRUE, PC-DMIS NC uses the macros supplied by the probe or NC manufacturer. Two macros are normally used:

- The first macro measures the size and location of a known (size and position) hole. The size of the hole is used to determine the diameter of the probe. The location of the hole determines the offsets of the probe center from the spindle axis.

- The second macro determines the probe tool length by touching a flat surface that is perpendicular to the spindle axis and whose location is known with respect to the spindle gage point. Follow your existing documentation for information on how to do this.

Entry Name: IncludeUtilMacros

Entry Type: True/False value. Default value is TRUE.