Current Help System: PC-DMIS Settings Editor (View Core Help)

Machine Interface Settings

The Settings Editor has sections that are visible depending on the Machine Interface that is loaded with PC-DMIS. These sections will not be discussed as part of this documentation, but are discussed as part of the Machine Interface Installation Manual (MIIM). The values under the following sections are discussed in the MIIM:

Axila B&S_Embedded_Board_Interface Backtalk_Interface (Brown & Sharpe) Bright (Mitutoyo Euro-c) Coord3-PMAC

DEA_Interface

ELMDRIVER (Elm & Starrrett)

Faro_Interface

FEDERAL

GARDA

GOM (CTR & Krypton)

JOHANSSON

Iplusplus

Leica

LEITZ

LKDRIVER

LK Direct

MANMITI (Manual Mitutoyo)

MANMORA (Manual MORA)

METROLOG (Metrologic)

METROMEC

Mitutoyo

MORA

MZEISS (Manual Zeiss)

NUMEREX

Old_Dea

OmniMan (Manual Omnitech)

OMNITECH

POLAR

PROFTECH (Profitech)

REFLEX

RENISHAW

Romer_Interface

SHARPE32

Sheffield

SMX Laser Interface

Tech80_Interface

Theodolite_Interface

WENZEL

ZEISS

Important: Values related to the Machine Interface should only be altered by a trained technician