Current Help System: PC-DMIS Settings Editor (View Core Help)

### End Angle

Allows you to define the default value for the End Ang option that will be used when an Auto Feature is created. This is a user supplied angle in decimal degrees. This value is used for Vision probes while the "DccEndAng" value is used for Contact probes.

Entry Name: EndAngle

Entry Type: Real Number to specify the angle in degrees. Default value is 0.

Note: It is important to remember when entering starting and ending angles that the IJK vector always looks down the centerline, and that PC-DMIS measures DCC circular features in a counterclockwise direction.