Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Shutter Time To Fire Stage Drift

This value provides the delay (in milliseconds) that PC-DMIS waits before firing of the point detection command when a stage drift has been detected.

This value is only evaluated when "AutoShutterEnable" is set to TRUE (1). If the stage is not stable, then point detection is not reliable.

Entry Name: AutoShutterTimeToFireStageDrift

Entry Type: Whole Number to specify milliseconds. Default value is 2000.