Current Help System: PC-DMIS Settings Editor (View Core Help)

### Back Off

This value is used with Flush and Gap Laser Auto Feature. The back-off distance determines the location from the gap’s edge at which PC-DMIS measures the flush distance. This distance is measured from the edge of the gap.

Entry Name: BackOff

Entry Type: Real Number to specify distance. Default value is 0.

required to change entry