Current Help System: PC-DMIS Settings Editor (View Core Help)

### Auto Adjust Probe Max Angle

Provides the maximum angle allowed between the part surface and the laser probe. It is used to decide when a different tip angle is needed for scanning. In a scan it’s best that the machine motion is such that the stripe on the part is perpendicular to the machine motion. If it is greater than this value a new tip angle is selected.

Entry Name: AutoAdjustProbeMaxAngle

Entry Type: Real Number to specify angle in degrees. Default value is 45.