Current Help System: PC-DMIS Settings Editor (View Core Help)

### Update Meas Vals after Iterative Alignment

This entry determines whether or not measured values of measured points, auto vector points, and auto surface points are updated after the iterative alignment solves.

Entry Name: UpdateMeasValsAfterIterativeAlignment

Entry Type: Boolean value. The default value is TRUE.

- If set to TRUE, PC-DMIS updates the measured values of the features after the alignment solves. This is the default behavior and is the way PC-DMIS behaved from version 3.25 to the current version. Prior to 3.25 we did not update the measured values. Only measured points, auto vector points, and auto surface points will have their values updated.

- If the value is FALSE, then the measured values are not adjusted by the alignment.