Current Help System: PC-DMIS Settings Editor (View Core Help)

### Minimum Tip Orientations for Size Averaging

This entry lets you specify the minimum number of validly calibrated tip orientations that must be present for averaging to take place. Even if the Use tip size averaging check box is marked in the Probe Setup dialog box, you must still have the minimum number of validly calibrated tip orientations.

Allows you to indicate the percentage of the sphere you want to cover. The general recommendation is 70%

Entry Name: MinimumTipOrientationsForSizeAveraging

Entry Type: Real Number specifying the minimum number of probe orientations that must be present for averaging to take place. The default value is 5 and can never go below 2.