Current Help System: PC-DMIS Settings Editor (View Core Help)

### Flush And Gap CG Gray Sum Min

Provides the minimum pixel intensity below which pixels exceeding this value will not be used. This value is used when measuring laser flush and gap features using the Gray Sum locater type.

Entry Name: FlushAndGap_CGGraySumMin

Entry Type: Whole Number specifying minimum pixel intensity. Default value is 30.