Current Help System: Tutor Translator (View Core Help)

### Middle Point Measurement Commands

PC-DMIS does not have an equivalent measurement command. Middle point can only constructed using a set of measured points. The command is translated as a measure SET command and a construction command.

MMIDPT (MEMORY [27], 2) path PT27 translates to è

ASSIGN/E.BADMEAS=0

SCN1 = FEAT/SET,RECT

THEO/<2.5,20,34.5>,<0,0,1>
ACTL/<2.5,20,34.5>,<-0.3582638,0,-0.9336204>
MEAS/SET,2
MOVE/POINT,<20,20,30>
HIT/BASIC,<10,20,39>,<10,20,39>,USE THEO = NO
MOVE/POINT,<20,30,30>
MOVE/POINT,<-15,30,30>
MOVE/POINT,<-15,20,30>
HIT/BASIC,<-5,20,30>,<-5,20,30>,USE THEO = NO
MOVE/POINT,<30,30,30>
ENDMEAS/

PNT12 = FEAT/POINT,RECT

THEO/<2.5,20,34.5>,<0,0,1>
ACTL/<2.5,20,34.5>,<0,0,1>
CONSTR/POINT,MID,SCN1.HIT[1],SCN1.HIT[2]
ASSIGN/E.WM2 = E.WM1
ASSIGN/E.WM1 = TUTORELEMNT("PNT12")
ASSIGN/E.MEMORY[20] = E.WM1
…
… Evaluation commands.
…